/* DATA DESCRIPTION:
Citation:	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Zielinski, Oliver (2020): Hyperspectral above-water radiometric quantities observed during cruise SO267/2 aboard RV SONNE [dataset bundled publication]. PANGAEA, https://doi.org/10.1594/PANGAEA.924038
Abstract:	Automated continuous above-water hyperspectral calibrated radiometric quantities were observed in the international waters of the Pacific Ocean during the scientific field campaign SO267/2 aboard RV SONNE. The cruise began on 28 January 2019 from Suva, Fiji and finished on 14 February 2019 in Manzanillo, Mexico. A radiometer setup with two TriOS RAMSES-ACC hyperspectral cosine irradiance meters to measure incoming solar irradiance, four TriOS RAMSES-ARC hyperspectral radiance meters to measure total upward sea surface leaving radiance Lsfc at 45° nadir and sky-leaving radiance Lsky at 45° zenith angle were installed using a custom-made frame at the bow of RV SONNE. The frame was attached to the bow of the ship with the radiance meters having a 90° azimuthal angle separating them or 45° from the ship heading/bow. Quality control involved retaining the Lsfc observations with lowest values (Garaba et al., 2012; Garaba et al., 2015). Data logging was automated using TriOS MSDA XE version 8.9.2 software and further processing was done using Mathworks Matlab 2016a and R software. Processed data was interpolated to 1 nm spectral resolution using PCHIP function in Matlab between 320 and 950 nm. Raw data is available on request.
Keyword(s):	hypespectral; Pacific Ocean; radiometric quantities; RV Sonne; SO267/2
Supplement to:	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Zielinski, Oliver (in prep.): Hyperspectral above-water radiometric quantities observed during cruise SO267/2 aboard RV SONNE.
Further details:	Garaba, Shungudzemwoyo Pascal; Schulz, Jan; Wernand, Marcel Robert; Zielinski, Oliver (2012): Sunglint Detection for Unmanned and Automated Platforms. Sensors, 12(9), 12545-12561, https://doi.org/10.3390/s120912545
	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Wollschläger, Jochen; Zielinski, Oliver (2015): Modern approaches to shipborne ocean color remote sensing. Applied Optics, 54(12), 3602-3612, https://doi.org/10.1364/AO.54.003602
Project(s):	Institut für Chemie und Biologie des Meeres (ICBM) (URI: https://uol.de/icbm)
Coverage:	MEDIAN LATITUDE: 7.152612 * MEDIAN LONGITUDE: -128.940274 * SOUTH-BOUND LATITUDE: -2.607549 * WEST-BOUND LONGITUDE: -150.395014 * NORTH-BOUND LATITUDE: 16.990388 * EAST-BOUND LONGITUDE: -107.064668
	DATE/TIME START: 2019-02-03T16:52:40 * DATE/TIME END: 2019-02-13T18:35:00
License:	Creative Commons Attribution 4.0 International (CC-BY-4.0) (URI: https://creativecommons.org/licenses/by/4.0/)
Size:	3 datasets
*/
/* TABULAR SUMMARY OF DATASETS LISTED IN THIS COLLECTION: */
Filename	Citation of child dataset
SO267-2_Ed.tab	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Zielinski, Oliver (2020): Hyperspectral downward irradiance observed during cruise SO267/2 aboard RV SONNE. https://doi.org/10.1594/PANGAEA.923910
SO267-2_Lsfc.tab	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Zielinski, Oliver (2020): Hyperspectral total upward sea surface leaving radiance observed at 45° nadir angle during cruise SO267/2 aboard RV SONNE. https://doi.org/10.1594/PANGAEA.924005
SO267-2_Lsky.tab	Garaba, Shungudzemwoyo Pascal; Voß, Daniela; Zielinski, Oliver (2020): Hyperspectral downward sky leaving radiance observed at 45° zenith angle during cruise SO267/2 aboard RV SONNE. https://doi.org/10.1594/PANGAEA.924035
