/* DATA DESCRIPTION:
Citation:	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations within DynaCom experimental islands and saltmarsh enclosed plots at different elevation levels, Spiekeroog, Germany, 2020-01 to 2023-09 [dataset publication series]. PANGAEA, https://doi.org/10.1594/PANGAEA.989251
Abstract:	Data presented here were collected between January 2020 to September 2023 within the research unit DynaCom (Spatial community ecology in highly dynamic landscapes: From island biogeography to metaecosystems, https://uol.de/dynacom/ ) involving the Universities of Oldenburg, Göttingen, and Münster, the iDiv Leipzig and the Nationalpark Niedersächsisches Wattenmeer. Experimental islands and saltmarsh enclosed plots were established in the back-barrier tidal flat and in the saltmarsh zone of the island of Spiekeroog (Germany). Groundwater levels at different elevation zones were measured using pressure loggers deployed in dip wells within the experimental islands as well as in the saltmarsh enclosed plots. Measurements were obtained using Hobo U20L Water Level Loggers (Onset Computer Corporation, Bourne, MA/USA) and a DEFI-D Miniature Pressure Recorder (JFE Advantech Co., Ltd., Tokyo; DEFI-D). All devices were pre-calibrated by the manufacturer. Logged data were retrieved in the field using a Hobo Underwater Shuttle (U-DTW-1) and were read out with the HOBOware Pro (V3.7.28) software or with the DEFI Series software (V1.02), depending on the instrument. Subsequent data processing was done using MATLAB (R2024b). Atmospheric pressure correction for water-level calculations was applied using data from a nearby weather station. Post-processing and quality control included (a) the removal of data covering maintenance activities, (b) an outlier detection, and (c) visual checks. Outliers in water level and temperature time series were detected using a moving-median filter and a 3-sigma criterion, with additional cross-checking against a reference sensor. Identified outliers were removed, and height-corrected water level series were produced to ensure consistency across sensors and years.
Keyword(s):	BEFmate; biodiversity - ecosystem functioning; DynaCom; experimental islands; Field experiment; groundwater level; Metacommunity; salt marsh; Spiekeroog; water level
Related to:	Meier, Daniela; Thölen, Claudia; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Zielinski, Oliver (2020): Continuous water level observations within DynaCom experimental islands and saltmarsh enclosed plots at different elevation levels (2019), Spiekeroog, Germany, 2019-01 to 2019-12 [dataset publication series]. Institute for Chemistry and Biology of the Marine Environment, Carl von Ossietzky University Oldenburg, Germany, PANGAEA, https://doi.org/10.1594/PANGAEA.920175
References:	Zielinski, Oliver; Meier, Daniela; Lõhmus, Kertu; Balke, Thorsten; Kleyer, Michael; Hillebrand, Helmut (2018): Environmental conditions of a salt-marsh biodiversity experiment on the island of Spiekeroog (Germany). Earth System Science Data, 10(4), 1843-1858, https://doi.org/10.5194/essd-10-1843-2018
Project(s):	FOR 2716: Spatial community ecology in highly dynamic landscapes: from island biogeography to metaecosystems (DynaCom) (URI: https://uol.de/en/icbm/collaborative-projects/dynacom)
Funding:	German Research Foundation (DFG) (URI: http://www.dfg.de/en/), grant/award no. 379417748: FOR 2716: Spatial community ecology in highly dynamic landscapes: from island biogeography to metaecosystems (URI: https://gepris.dfg.de/gepris/projekt/379417748)
Coverage:	MEDIAN LATITUDE: 53.759638 * MEDIAN LONGITUDE: 7.722012 * SOUTH-BOUND LATITUDE: 53.757314 * WEST-BOUND LONGITUDE: 7.717647 * NORTH-BOUND LATITUDE: 53.762633 * EAST-BOUND LONGITUDE: 7.724789
	DATE/TIME START: 2020-01-01T00:00:00 * DATE/TIME END: 2023-09-02T23:50:00
License:	Creative Commons Attribution 4.0 International (CC-BY-4.0) (URI: https://creativecommons.org/licenses/by/4.0/)
Size:	12 datasets
*/
/* TABULAR SUMMARY OF DATASETS LISTED IN THIS COLLECTION: */
Filename	Citation of child dataset
DynaCom_GWlvl_20-23_I3low.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I3low, 2020-01 to 2022-05. https://doi.org/10.1594/PANGAEA.989252
DynaCom_GWlvl_20-23_I3upp.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I3upp, 2020-01 to 2023-04. https://doi.org/10.1594/PANGAEA.989317
DynaCom_GWlvl_20-23_I4low.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I4low, 2020-01 to 2023-04. https://doi.org/10.1594/PANGAEA.989318
DynaCom_GWlvl_20-23_I4pio.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I4pio, 2020-01 to 2023-03. https://doi.org/10.1594/PANGAEA.989319
DynaCom_GWlvl_20-23_I4upp.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I4upp, 2020-01 to 2021-07. https://doi.org/10.1594/PANGAEA.989320
DynaCom_GWlvl_20-23_I10low.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I10low, 2020-01 to 2023-06. https://doi.org/10.1594/PANGAEA.989314
DynaCom_GWlvl_20-23_I10pio.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I10pio, 2020-01 to 2023-01. https://doi.org/10.1594/PANGAEA.989315
DynaCom_GWlvl_20-23_I10upp.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_I10upp, 2020-01 to 2023-09. https://doi.org/10.1594/PANGAEA.989316
DynaCom_GWlvl_20-23_S3low.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_S3low, 2020-01 to 2023-09. https://doi.org/10.1594/PANGAEA.989324
DynaCom_GWlvl_20-23_S10low.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_S10low, 2020-01 to 2021-04. https://doi.org/10.1594/PANGAEA.989321
DynaCom_GWlvl_20-23_S10pio.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_S10pio, 2020-01 to 2023-09. https://doi.org/10.1594/PANGAEA.989322
DynaCom_GWlvl_20-23_S10upp.tab	Pieck, Daniela; Schwalfenberg, Kai; Weyel, Niklas; Hillebrand, Helmut; Kleyer, Michael; Lõhmus, Kertu; Wollschläger, Jochen; Zielinski, Oliver; Badewien, Thomas Henry (2026): Continuous water level observations at station BEFmate_S10upp, 2020-01 to 2023-09. https://doi.org/10.1594/PANGAEA.989323
